COLUMN		DATA ELEMENT		DESCRIPTION
______		____ _______		___________

1		AIRFRAME TYPE		0 = cessna 182 RG
					1 = schweizer 2-32
					2 = learjet 35
					3 = sopwith camel
					4 = experimental cessna
					5 = experimental fighter jet
					6 = experimental glider

2		BLANK

3		2D GRAPHICS DRIVER	V = 320x400x256-color VGA
					S = 640x400x256-color Super VGA
					E = 640x350x16-color EGA
					M = 640x350xmono EGA

4		BLANK

5-?		.PNL FILE NAME		THIS FIELD IS TEMINATED BY THE FIRST
					<SPACE> (20h) OR <TAB> (09h)
					ENCOUNTERED.  (OR BY THE LINE ENDING
					<CR> <LF>.)

REST OF LINE	COMMENT			OPTIONAL.  MUST BE SEPERATED FROM THE
					PRIVEOUS FIELD BY 'WHITE SPACE.'


Note: Each line is terminated by a <CARRIAGE RETURN> and <LINE FEED>.


&	      	The first '&' marks the last line before the data begins
0 V CESN_V	panels\cesn_v.pnl
0 S CESN_S
0 E CESN_E
0 M CESN_M
1 V SCHW_V
1 S SCHW_S
1 E SCHW_E
1 M SCHW_M
2 V LEAR_V
2 S LEAR_S
2 E LEAR_E
2 M LEAR_M
3 V SOPW_V
3 S SOPW_S
3 E SOPW_E
3 M SOPW_M
4 V CESN_V	panels\cesn_v.pnl
4 S CESN_S
4 E CESN_E
4 M CESN_M
5 V LEAR_V
5 S LEAR_S
5 E LEAR_E
5 M LEAR_M
6 V SCHW_V
6 S SCHW_S
6 E SCHW_E
6 M SCHW_M
&		The first '&' after the data begins marks end of the data.

